Text for specification

Description
double-T section busbar 500 mm²
length 653 mm, tinned
60Classic
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
power dissipation at full load of the item:	43,3 W

diagram current capacity (IEC) 

Material properties
Main body:
	Cu-ETP R300 (EN 13601), tinned

corrosion-resistant, also in aggressive environments

Miscellaneous 
Tin-plated Cu busbars considerably reduce the effort of preparing the contact points.
The Cu busbars are effective protected against aggressive media.

Brand 
Woehner or equivalent

Part No.
01226000