Text for specification

Description
clip-on screw connection, for cable lugs
M10
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	0,5 W
current capacity (IEC) max.:	630 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  I_pk max.:	59,7 kA

Terminal points
Suitable for aluminium cables.
When using aluminium cables, observe the maintenance instructions.

Material properties
Connecting screws:
	Hexagon screw M10, length across flats 17
Terminal body:
	steel, galvanized and chromized

Terminal body: nickel-plated Cu section
screw: hexagon screw with slot, galvanised, chromited

Brand 
Woehner or equivalent

Part No.
01749000