Text for specification

Description
CRITO®
profile terminal
500 - 750 mm²
terminal space 51 x 5-28
60Classic
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	1.600 A
rated voltage (IEC) AC:	690 V

rated current (UL):	1.200 A
rated voltage (UL) AC:	600 V
current carrying capacity for centre feed:	1.600 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	81,9 kA

SCCR:	25 kA

Terminal points
terminal space 51 x 5-28
1 terminal screw M12

Material properties
Connecting screws:
	Set screw M16, Allan key size 8

Stainless steel terminal body

Miscellaneous 
also rigid copper busbars can be connected if they are installed without mechnical tension 

Brand 
Woehner or equivalent

Part No.
01906000