Text for specification

Description
1-pole comb-type busbar, for E27, pitch 40 mm
80 A, 1 m long
16 mm²
Accessories

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	80 A
rated voltage (IEC) AC:	400 V

power dissipation at full load of the item:	2,8 W
current carrying capacity for centre feed:	130 A
rated surge voltage Uimp :	4 kV

Brand 
Woehner or equivalent

Part No.
31309000A