Text for specification

Description
EQUES®60Classic
busbar adapter 32 A
for direct starter Siemens 3RA6
45 x 200, with leads AWG 10 (6 mm²), with metal mounting rail
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	32 A
rated voltage (IEC) AC:	690 V

rated current (UL):	32 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	2,5 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 30 kA with S0 12,5 A / 600 V AC, 65 kA with S0 16 A / 480 V AC, 65 kA with S0 25 A / 480 V AC, 50 kA with S0 32 A / 480 V AC 

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32588000