Text for specification

Description
EQUES^®30Compact
busbar adapter 30 A
for direct starter Siemens S0 with spring terminal connection
45 x 160, with leads AWG 10 (6 mm²)
30Compact 3P

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	30 A
rated voltage (IEC) AC:	690 V

rated current (UL):	30 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	2,5 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

SCCR: 65 kA with any NKJH Comb. Motor Controller 16 A / 480 V AC, 65 kA with any NKJH Comb. Motor Controller 25 A / 480 V AC, 30 kA with any NKJH Comb. Motor Controller 12,5 A / 600 V AC, 50 kA with any NKJH Comb. Motor Controller 32 A / 480 V AC 

Material properties
Conductor insulation: 	temperature-resistant up to 105 °C

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32694000A