Text for specification

Description
current transformer 600 A / 5 A
2.5 VA / class 0.5s
60Classic
Accessories

Standards
IEC 61869-1:2007
IEC 61869-2:2012

Electrical data
power dissipation at full load of the item:	4,0 W

Terminal points
cage clamp connection
screw drive: PZ1 
wire stripping: 12 mm
min. cross-section: 2,5 mm²
max. cross-section: 4 mm²
cage clamp connection
screw drive: PZ1 
wire stripping: 12 mm
min. cross-section: 2,5 mm²
max. cross-section: 4 mm²
Md min.: 2,0 Nm
Md max.: 2,0 Nm
Not suitable for aluminium cables !

Brand 
Woehner or equivalent

Part No.
37229000A