Text for specification

Description
flexible copper busbar, tinned, insulated
5x 40 x 1
736 A, length 2 m
Accessories

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	736 A

power dissipation at full load of the item:	114,1 W

Miscellaneous 
Tin-plated Cu bars considerably reduce the effort of preparing the contact points.
The Cu busbars are effectively protected against aggressive media.

Brand 
Woehner or equivalent

Part No.
01097000