Text for specification

Description
CRITO^®60Classic
connection module
with integrated spring terminals 1.5 - 16 mm², AWG 14 - 6
3-pole
60Classic

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
UL

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	690 V

rated current (UL):	48 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	80 A

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV
max. permitted voltage (IEC) AC:	800 V
max. permitted voltage (IEC) DC:	800 V

rated peak withstand current  I_pk max.:	13 kA

SCCR: 35 kA with any DIVQ/7 circuit breaker 60 A / 480 V AC , 50 kA with JDDZ fuse Class J 60 A / 600 V AC 

Terminal points
for leads as per IEC :
Cu 1.5 - 16mm²
round conductor solid or stranded, flexible, direct or with wire-end ferrule

for leads as per UL :
Cu AWG 14 - 6
Class B (UL486E)

Brand 
Woehner or equivalent

Part No.
01563000A