Text for specification

Description
neutral conductor 160 A
clamp, both sides

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	160 A
rated voltage (IEC) AC:	690 V
rated voltage (IEC) DC:	440 V

power dissipation at full load of the item:	8,0 W
max. permitted voltage (IEC) AC:	800 V
max. permitted voltage (IEC) DC:	800 V

Brand 
Woehner or equivalent

Part No.
03620000