Text for specification - draft 

Description
CAPUS®Panel
switch-disconnector 2-pole
screw M10, without handle
400 A

Standards
IEC 60947-1:2020
IEC 60947-3:2020

Approvals
UL

Electrical data

rated current (UL):	400 A
rated voltage (UL) DC:	1500 V

power dissipation at full load of the item:	11,0 W

Gebrauchskategorien siehe Datenblatt (unter Downloads) 

Brand 
Woehner or equivalent

Part No.
23051000AD