Text for specification

Description
EQUES®60Classic
busbar adapter 80 A
for circuit breaker Siemens HGG, LGG, NGG
81 x 200, with leads AWG 4 (25 mm²), with metal plate
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	80 A
rated voltage (IEC) AC:	690 V

rated current (UL):	80 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	7,3 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 14 kA with Siemens NGG, HGG, LGG 125 A / 600 V AC, 65 kA with Siemens NGG, HGG, LGG 125 A / 480 V AC 

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32029000A