Text for specification

Description
EQUES^®60Classic
busbar adapter 650 A, 3-pole
238 x 300
60Classic

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	650 A
rated voltage (IEC) AC:	690 V

rated current (UL):	640 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	63,0 W

rated isolation voltage U_i AC:	1000 V
rated surge voltage U_imp :	6 kV
max. permitted voltage (IEC) AC:	800 V

SCCR: 42 kA with 140G-M / 600 V AC, 65 kA with T6 / 480V AC, 65 kA with 3RV1083 / 480V AC, 65 kA with 140G-M / 480V AC 

Brand 
Woehner or equivalent

Part No.
32064000A