Text for specification

Description
CAPUS®Panel
PE terminal for SD1-3P switch-disconnector

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
UL

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	690 V

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	4 kV
rated making capacity:	2,1 kA

Brand 
Woehner or equivalent

Part No.
33689000A