Text for specification

Description
centre feed unit 1250 A
for cabinet width 800 mm
centre feed unit

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	1.250 A
rated voltage (IEC) AC:	690 V

rated current (UL):	1.200 A
rated voltage (UL) AC:	480 V

power dissipation at full load of the item:	66,8 W

rated isolation voltage U_i AC:	1000 V
rated surge voltage U_imp :	8 kV

rated peak withstand current  I_pk max.:	84 kA

4-pole busbar system, can be retrofitted

Miscellaneous 
Clear construction and undrilled connection technology enable safe and cost-efficient solutions to problems.

Brand 
Woehner or equivalent

Part No.
35006000