Text for specification

Description
EQUES®60Classic
busbar adapter 630 A
Anschlussschrauben M10 (oben / unten)
184 x 320
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	630 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	31.5 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) DC:	800 V

Material properties
Mounting plate: 	plastic

Brand 
Woehner or equivalent

Part No.
32004000