Text for specification

Description
CRITO®
brace terminal
600 - 1200 mm²
terminal space 68 x 28
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2020

Approvals
UL

Electrical data
Rated current (IEC):	1,600 A
rated voltage (IEC) AC:	690 V

rated current (UL):	1,400 A
rated voltage (UL) AC:	600 V
current carrying capacity for centre feed:	2,000 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	80 kA

SCCR: 200 kA with fuse Class L 1600 A, 65 kA with any DIVQ/7 circuit breaker 1600 A / 480 V AC/DC 

Miscellaneous 
also rigid copper busbars can be connected if they are installed without mechnical tension 

Brand 
Woehner or equivalent

Part No.
01070000