Text for specification

Description
CRITO^®
brace terminal
1000 - 2000 mm²
terminal space 105 x 28
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	1,600 A
rated voltage (IEC) AC:	690 V

rated current (UL):	1,800 A
rated voltage (UL) AC:	600 V
current carrying capacity for centre feed:	2,800 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  I_pk max.:	85.5 kA

SCCR: 65 kA with any DIVQ/7 circuit breaker 2500 A / 480 V AC/DC, 65 kA with any DIVQ/7 circuit breaker 1600 A / 480 V AC/DC, 200 kA with fuse Class L 1600 A 

Miscellaneous 
also rigid copper busbars can be connected if they are installed without mechnical tension 

Brand 
Woehner or equivalent

Part No.
01071000