Text for specification

Description
busbar connecting terminal 520 A
55 mm
30Compact 3P
60Classic

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	3.9 W
current capacity (IEC) max.:	520 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  I_pk max.:	63.1 kA

Brand 
Woehner or equivalent

Part No.
01166000