Text for specification

Description
CAPUS®Panel
changeover switch 3-pole
screw M12
1600 A

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Electrical data
Rated current (IEC):	1,600 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	112.8 W

rated isolation voltage Ui AC:	1000 V
rated surge voltage Uimp :	12 kV

Brand 
Woehner or equivalent

Part No.
23166000AD