Text for specification

Description
EQUES®CrossBoard
adapter 16 A
phase L3, 1 fixed mounting rail, with leads AWG 14 (2.5 mm²)
18 x 160

Standards
IEC 61439-1:2020

Approvals
UL

Electrical data
Rated current (IEC):	16 A
rated voltage (IEC) AC:	690 V

rated current (UL):	16 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	1.0 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 14 kA with any DIVQ/7 circuit breaker 16 A / 480 V AC, 65 kA with any 3-pole NKJH/7 Comb. Motor Controller 16 A / 480 V AC, 65 kA with any 1-pole NKJH/7 Comb. Motor Controller 16 A / 277 V AC, 50 kA with JFFZ fuse Class CC 20 A / 600 V AC 

Brand 
Woehner or equivalent

Part No.
32302000A