Text for specification

Description
EQUES^®CrossBoard
adapter 32 A
1 adjustable mounting rail, with leads AWG 10 (6 mm²) 160 mm long,  for devices with spring terminal technology
45 x 160

Standards
IEC 61439-1:2011

Approvals
IEC (CB), UL

Electrical data
Rated current (IEC):	32 A
rated voltage (IEC) AC:	690 V

rated current (UL):	30 A
rated voltage (UL) AC:	600 V

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	6 kV

Miscellaneous 
Conductor ends ultrasonic compressed.
Click mechanism when pushing onto the CrossBoard®.

Brand 
Woehner or equivalent

Part No.
32686000A