Text for specification

Description
MOTUS®CrossBoard
hybrid motor starter, 3-pole
electronic unit direct and reversing starter 1.5 - 6.5 A / switch for resistive loads 1.5 - 9.0 A

Standards
EN 60947-1:2015
EN 60947-4-2:2012
EN 61439-1:2012
EN 50581:2012
EN ISO 13849-1:2015

Approvals
UL, CCC

Electrical data
Rated current (IEC):	9 A
rated voltage (IEC) AC:	500 V

rated current (UL):	6.5 A
rated voltage (UL) AC:	500 V

power dissipation at full load of the item:	12.0 W

rated isolation voltage Ui AC:	500 V
rated surge voltage Uimp :	6 kV

SCCR: 100 kA with JDDZ fuse Class J 175 A / 600 V AC  

Brand 
Woehner or equivalent

Part No.
36111000A