Text for specification

Description
PE-terminal, green/yellow
for bar 12 x 2
Accessories

Standards
IEC 60664-1:2007

Electrical data
Rated current (IEC):	63 A
rated voltage (IEC) AC:	400 V

rated isolation voltage Ui AC:	500 V
rated surge voltage Uimp :	6 kV

Material properties
Main body:
	temperature stability 125°C, 
	self-extinguishing in acc. to UL 94, 
	creepage resistance CTI 200
	halogen-free

Brand 
Woehner or equivalent

Part No.
01144000