Text for specification

Description
busbar terminal for longitudinal connection
38 mm long
60Classic

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V

rated current (UL):	1’400 A
rated voltage (UL) AC:	600 V
rated voltage (UL) DC:	600 V

power dissipation at full load of the item:	5.4 W
current capacity (IEC) max.:	1’600 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

SCCR: 35 kA with any DIVQ/7 circuit breaker 1600 A / 480V AC/DC 

Brand 
Woehner or equivalent

Part No.
01102000