Text for specification

Description
CRITO^®
profile terminal
1200 - 3600 mm²
terminal space 101 x 23-45
60Classic
185mm-System
centre feed unit

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	2’500 A
rated voltage (IEC) AC:	800 V

rated current (UL):	1’800 A
rated voltage (UL) AC:	600 V
current carrying capacity for centre feed:	3’200 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  I_pk max.:	107 kA

SCCR:	25 kA

Terminal points
terminal space 101 x 23-45
2 terminal screws M12

Miscellaneous 
also rigid copper busbars can be connected if they are installed without mechnical tension 

Brand 
Woehner or equivalent

Part No.
01186000