Text for specification

Description
PE/N-support
1-pole, attachable to 01500 or separate mounting
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
rated voltage (IEC) AC:	690 V
rated voltage (UL) AC:	600 V

rated isolation voltage U_i AC:	1000 V
rated surge voltage U_imp :	6 kV
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

Brand 
Woehner or equivalent

Part No.
01489000