Text for specification

Description
universal busbar support UL
3-pole, with internal screw holes
60Classic

Standards
IEC 61439-1:2020

Approvals
CSA, UL

Electrical data
rated voltage (IEC) AC:	800 V
rated voltage (UL) AC:	600 V

rated isolation voltage Ui AC:	1000 V
rated surge voltage Uimp :	8 kV
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	70 kA

go to calculation for  3-pole system (IEC) 

Brand 
Woehner or equivalent

Part No.
01508000