Text for specification

Description
cylindr. fuse link 4 A
500 V, gG
10 x 38
Accessories

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-2:2013 + A1:2016, Fuse system F

Electrical data
Rated current (IEC):	4 A
rated voltage (IEC) AC:	500 V

power dissipation at full load of the item:	0.8 W

rated short-circuit breaking capacity AC:	120 kA

Brand 
Woehner or equivalent

Part No.
31183000