Text for specification

Description
connection terminal, front connection
6 - 35 mm²
Accessories

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
Rated current (IEC):	115 A
rated voltage (IEC) AC:	1000 V

rated current (UL):	115 A
rated voltage (UL) AC:	1000 V
rated voltage (UL) DC:	1000 V
rated surge voltage Uimp :	4 kV
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1000 V

SCCR: 100 kA with fuse Class J 200 A 

Terminal points
6 - 35mm²
6Nm
max. connection diameter 11mm
AWG 10 - 1/0

Brand 
Woehner or equivalent

Part No.
31550000