Text for specification

Description
EQUES 60Classic
busbar adapter 32 A
1 adjustable mounting rail
54 x 200, with leads AWG 10 (6 mm²)
60Classic

Standards
IEC 61439-1:2020

Approvals
CSA, UL

Electrical data
rated current (IEC):	32 A
rated voltage (IEC) AC:	690 V

rated current (UL):	30 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	2.4 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 65 kA with any NKJH/7 Comb. Motor Controller type E 32 A / 480 V AC, 65 kA with any DIVQ/7 circuit breaker 40 A / 480 V AC 

Miscellaneous 
Conductor ends ultrasonically sealed.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32441000