Text for specification

Description
EQUES®60Classic
busbar adapter 580 A, 3-pole
184 x 325
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	580 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	83.4 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) DC:	800 V

Brand 
Woehner or equivalent

Part No.
32980000