Text for specification

Description
CAPUS®Panel
switch-disconnector 3-pole + N
box terminal 2.5 - 16 mm² / WG 16 - 6, yellow-red handle
16 A

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Approvals
UL

Electrical data
Rated current (IEC):	16 A
rated voltage (IEC) AC:	690 V

rated current (UL):	16 A
rated voltage (UL) AC:	600 V

AC-23 A (690 V / 16 A)
AC-22 A (690 V / 16 A)
AC-21 A (690 V / 16 A)

power dissipation at full load of the item:	0.4 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	4 kV
rated making capacity:	2.1 kA

Terminal points
für Anwendungen nach IEC / EN :
2,5 - 16 mm² rund eindrähtig, feindrähtig und feindrähtig mit Aderendhülse
16 mm² rund mehrdrähtig
Md 2 Nm

für Anwendungen nach UL / CSA :
AWG 16 - 6
17,7 lb-in

Miscellaneous 
lockable in 0-position with a padlock (max. 4 mm diameter) 

Brand 
Woehner or equivalent

Part No.
33839000A