Text for specification

Description
CRITO^®
terminal for flat conductors
40 x 25
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Electrical data
rated voltage (IEC) AC:	690 V
current capacity (IEC) max.:	1’250 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  I_pk max.:	80.9 kA

Material properties
Connecting screws:
	Set screw M16, Allan key size 8
Terminal body:
	steel, galvanized and chromized

Terminal body: 	brass, nickel-plated, screw: 	hexagon socket screw, galvanised, chromited

Miscellaneous 
Indication of nominal cross-section and tightening torque marked on the terminal.
Terminal can be subsequently fitted onto and removed from mounted busbar.

Brand 
Woehner or equivalent

Part No.
01092000