Text for specification

Description
connection terminal, front connection
25 - 95 mm²
Accessories

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	225 A
rated voltage (IEC) AC:	690 V
rated surge voltage Uimp :	4 kV
max. permitted voltage (IEC) AC:	690 V
max. permitted voltage (IEC) DC:	1000 V

1000V DC*
*The use of single-pole devices is determined exclusively by the installation conditions with regard to the insulation properties.

Terminal points
25 - 90mm² round, solid and stranded
25 - 70mm² flexible with wire-end ferrule
Md 19Nm

Brand 
Woehner or equivalent

Part No.
01198000A