Text for specification

Description
busbar connecting terminal 2500 A
150 mm
60Classic
185mm-System

Standards
IEC 61439-1:2020

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V

rated current (UL):	1,800 A

power dissipation at full load of the item:	15.4 W
current capacity (IEC) max.:	2,500 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	97.3 kA

SCCR: 65 kA in combination with HH1140-L and any DIVQ/7 2500 A / 480 V AC 

Material properties
Screws:
	Hexagon screw M8, length across flats 13
Terminal body:
	Cu-ETP R300 (EN 13601), tinned

Terminal body: 	Cu section, nickel-plated, 	for bridging the system separation, screws: 	hexagonal screws M8 with slot, galvanised, chromited

Brand 
Woehner or equivalent

Part No.
01275000