Text for specification

Description
CRITO®
universal conductor terminal
16 - 70 mm², AWG 6 - 2/0
30Compact 3P
60Classic

Standards
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
CSA, UL

Electrical data
Rated current (IEC):	175 A
rated voltage (IEC) AC:	690 V

rated current (UL):	175 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	400 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	46.7 kA

Miscellaneous 
Terminal with integrated holding spring, captive clamping screw and opened terminal space.
Indication of nominal cross-section and tightening torque noted on the terminal.

Brand 
Woehner or equivalent

Part No.
01287000