Text for specification

Description
CRITO®
brace terminal
Cu / Al 95 - 185 mm²
60Classic
100Energy
185mm-System
centre feed unit

Standards
IEC 61439-1:2020
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
UL

Electrical data
Rated current (IEC):	300 A
rated voltage (IEC) AC:	690 V

rated current (UL):	310 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	500 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	55.8 kA

SCCR:	25 kA

Miscellaneous 
Terminal with captive clamp screws, conductor can be overlapped, indication of nominal cross-section and tightening torque noted on the terminal, contact between conductor and busbar via cable bed.

Brand 
Woehner or equivalent

Part No.
01318000