Text for specification

Description
busbar connecting terminal 1600 A
150 mm long
60Classic
185mm-System

Standards
IEC 61439-1:2011

Approvals
UL

Electrical data
rated voltage (IEC) AC:	690 V

rated current (UL):	1,400 A

power dissipation at full load of the item:	10.6 W
current capacity (IEC) max.:	1,600 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  I_pk max.:	72.7 kA

SCCR:	45 kA

Material properties
Screws:
	Hexagon screw M8, length across flats 13
Terminal body:
	Cu-ETP R300 (EN 13601), tinned

Terminal body: 	Cu section, nickel-plated, 	for bridging the system separation, screws: 	hexagonal screws M8 with slot, galvanised, chromited

Brand 
Woehner or equivalent

Part No.
01829000