Text for specification

Description
door coupling rotary drive

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Electrical data

Miscellaneous 
handle can be locked in position 0 (off) with up to three locks with shackle diameter 4 to 5 mm

Brand 
Woehner or equivalent

Part No.
23912000AD