Text for specification

Description
connecting set 1600 A (3-pole)
150 mm, flexible longitudinal connection
60Classic
185mm-System

Standards
IEC 61439-1:2011

Electrical data
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	38.4 W
current capacity (IEC) max.:	1,600 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

Material properties
terminal body: brass
screws: hexagonal socket screws M12, galvanised, chromited
connector: welded laminated copper

Brand 
Woehner or equivalent

Part No.
30322000