Text for specification

Description
connection terminal, front connection
6 - 50 mm²
Accessories

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	125 A
rated voltage (IEC) AC:	690 V
rated surge voltage Uimp :	4 kV
max. permitted voltage (IEC) AC:	690 V
max. permitted voltage (IEC) DC:	600 V

Terminal points
6 - 50mm² round, solid and stranded
4 - 35mm² flexible with wire-end ferrule
Md 3.5Nm
max. connection diameter 10mm

Brand 
Woehner or equivalent

Part No.
31085000A