Text for specification

Description
CUSTO®60Classic
D-fuse base, busbar mounted, 42mm
for busbar 10 mm, gauge ring
E 27 / 3P
60Classic

Standards
IEC 60269-1:2006 + A1:2009 + A2:2014
IEC 60269-3:2010 + A1:2013 + A2:2019

Electrical data
Rated current (IEC):	25 A
rated voltage (IEC) AC:	500 V
rated voltage (IEC) DC:	500 V

power dissipation at full load of the item:	1.2 W
rated surge voltage Uimp :	4 kV
max. permitted voltage (IEC) AC:	550 V
max. permitted voltage (IEC) DC:	525 V
short-circuit strength when protected by fuses:	50 kA

Contacting of the fuse links on the 	busbar via silvered copper plate

for fuse links and gauge rings as per DIN VDE 0636-3 IEC / HD 60269-3

Brand 
Woehner or equivalent

Part No.
31408000