Text for specification

Description
EQUES®60Classic
busbar component support
2 adjustable mounting rails
54 x 200, with removable upper section, without electrical connection
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
rated voltage (IEC) AC:	690 V
rated voltage (UL) AC:	600 V

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

Brand 
Woehner or equivalent

Part No.
32421000