Text for specification

Description
EQUES®60Classic
busbar adapter 80 A
1 adjustable mounting rail
54 x 200, without leads, with terminals 1.5 - 16 mm², front operated
60Classic

Standards
IEC 61439-1:2011

Electrical data
Rated current (IEC):	80 A
rated voltage (IEC) AC:	690 V

power dissipation at full load of the item:	9.3 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV
max. permitted voltage (IEC) DC:	800 V

Material properties
Conductor insulation: 	temperature-resistant up to 105 °C

Miscellaneous 
Free phase selection.
Click mechanism when pushing onto the busbar.

Brand 
Woehner or equivalent

Part No.
32464000