Text for specification

Description
EQUES®60Classic
busbar adapter 580 A, 3-pole
140 x 300
60Classic

Standards
IEC 61439-1:2011

Approvals
CSA, UL

Electrical data
Rated current (IEC):	580 A
rated voltage (IEC) AC:	690 V

rated current (UL):	630 A
rated voltage (UL) AC:	600 V

power dissipation at full load of the item:	75.0 W

rated isolation voltage Ui AC:	800 V
rated surge voltage Uimp :	6 kV

SCCR: 65 kA with Tmax T5 / 480 V AC, 65 kA with 3RV1073 / 480 V AC, 65 kA with 140G-K / 480 V AC 

Brand 
Woehner or equivalent

Part No.
32593000