Text for specification

Description
QUADRON^®Panel
NH fuse switch-disconnector size 4a, 1600 A, panel mounting
2x screw M12

Standards
IEC 60947-1:2020
IEC 60947-3:2020 AC ratings only

Electrical data
Rated current (IEC):	1,600 A
rated voltage (IEC) AC:	690 V

AC-22B (400V), AC-21B (690V)

DC-21B (440 V)

power dissipation at full load of the item:	240.0 W

rated isolation voltage U_i AC:	800 V
rated surge voltage U_imp :	8 kV

Terminal points
Flat connection (50mm wide) 2xM12

Material properties
Contacts:
externally tensioned copper contacts, silvered
screws:
hex-head screws, galvanised

Miscellaneous 
Disconnector is equipped with arc chambers.

Brand 
Woehner or equivalent

Part No.
33204000