Text for specification

Description
MOTUS®C14 CrossBoard Connect Plus
electronic motor starter, 3-pole or 1-pole switchable
direct and reversing starter 0.1 - 6.6 A
with IO-Link interface, with display

Standards
IEC 60947-1:2007 + A1:2010
IEC 60947-4-2:2011

Approvals
UL, CCC

Electrical data
Rated current (IEC):	6.6 A
rated voltage (IEC) AC:	500 V

rated current (UL):	6.6 A
rated voltage (UL) AC:	480 V

power dissipation at full load of the item:	20.0 W

rated isolation voltage Ui AC:	500 V
rated surge voltage Uimp :	4 kV

SCCR:	100 kA

Brand 
Woehner or equivalent

Part No.
36262000A