Text for specification

Description
flexible copper busbar, plain, insulated
4x 24 x 1
438 A, length 2 m
Accessories

Standards
IEC 61439-1:2020

Approvals
UL

Electrical data
Rated current (IEC):	438 A

power dissipation at full load of the item:	84.2 W

Miscellaneous 
The laminated Cu busbars considerably reduce the effort of connecting busbars. The bending devices required for solid copper busbars are unnecessary. The 2mm-thick insulation means that no additional covering is required.

Brand 
Woehner or equivalent

Part No.
01253000