Text for specification

Description
CRITO®
universal conductor terminal
1.5 - 16 mm², AWG 16 - 6
30Compact 3P
60Classic

Standards
IEC 61439-1:2011
IEC 60999-1:1999
IEC 60999-2:2003

Approvals
CSA, UL

Electrical data
Rated current (IEC):	65 A
rated voltage (IEC) AC:	690 V

rated current (UL):	65 A
rated voltage (UL) AC:	600 V
current capacity (IEC) max.:	180 A
max. permitted voltage (IEC) AC:	1000 V
max. permitted voltage (IEC) DC:	1500 V

rated peak withstand current  Ipk max.:	30.6 kA

Terminal points
1.5 - 16 mm² / AWG 14 - AWG 6 
flexible cables, directly or with wire-end ferrule, 
solid and stranded round cables, 
lam. Cu 8 x 6 x 0.5

(flexible cables of maximum cross-section may not fit when using wire-end ferrule)

Miscellaneous 
Terminal with integrated holding spring, captive clamping screw and opened terminal space.
Indication of nominal cross-section and tightening torque noted on the terminal.

Brand 
Woehner or equivalent

Part No.
01284000